# Additional info

## Matrix

You probably tried or will try to configure the keymapping to your liking. To make it easier configuring your layouts, photo of keyboards matrix will help.

![TMO50 matrix](https://i.imgur.com/ud7RB8d.png)

As you can see here matrix consists of 4 rows and 14 columns. But the tricky part is that topmost left key (Tab/Esc) is connected to row 3 - this is done so there's no 15th column that would connect only one key to seperate pin. This also poses an thread that you will configure your layout incorrectly because KC_TAB is not in the correct place *[visually](https://i.imgur.com/RtoD9F6.png)* in *keymap.c* file. Please take this into account when making changes and double-check this.

## Pinout

Most of the pinout can be found in *config.h* but there's here's a table of all the used pins for TMO50 (including indicator LED pins)

| Pin | Assigned to |
|---|---|
| D5 | Row 0 |
| D3 | Row 1 |
| D2 | Row 2 |
| D0 | Row 3 |
|    |       |
| D1 | Col 0 |
| D4 | Col 1 |
| F0 | Col 2 |
| F1 | Col 3 |
| F4 | Col 4 |
| F5 | Col 5 |
| F6 | Col 6 |
| F7 | Col 7 |
| D6 | Col 8 |
| D7 | Col 9 |
| B4 | Col 10 |
| B5 | Col 11 |
| B6 | Col 12 |
| C6 | Col 13 |
|    |        |
| B7 | Backlight |
| C7 | RGB LEDs |
| B0 | LED 4 (L4) |
| B1 | LED 3 (L3) |
| B2 | LED 2 (L2) |
| B3 | LED 1 (L1) |

## Indicator LEDs

Their size is 2×3×4mm. The THT hole without a circle on the pcb is VCC(+) and the other one is connect to their corresponding pin.
